For 1990-2009 cars

### Removal Procedure

1. Remove the front fender. Refer to Front Fender Replacement .
2. Release the pressure clips on the inner edge of the fender.
3. Remove the fender inner panel from the fender.

### Installation Procedure

1. Position the fender inner panel locator pin into the fender locator hole at the rear of the fender.
2. Install the fender inner panel pressure clips into the fender.
3. Install the front fender. Refer to Front Fender Replacement in this section.