For 1990-2009 cars

Complaint/Condition | Possible Cause(s) | Correction(s)
--- | --- | ---
Clicking noise in turn | Worn or damaged outer CV joint(s) | Replace outer CV joint(s).
CLUNK when accelerating from coast-to-drive | Worn or damaged inboard tri-pot joint(s) | Replace inboard tri-pot joint(s).
Shudder or vibration during acceleration | Excessive joint angle:

- Incorrect toe
- Incorrect bumper height

- Adjust toe.
- Correct bumper height.

| Worn or damaged inner or outer CV joint(s) | Replace inner or outer CV joint(s).
Vibration at highway speeds. | Out of balance wheel(s) or tire(s) | Balance wheel(s) or tire(s).
| Out of round wheel(s) or excessive radial force variation - Hard spot in tire(s) | Replace wheel(s) or tire(s).
| Worn CV joint(s) | Replace CV joint(s).
| Binding or tight CV joint(s) | Replace CV joint(s).