For 1990-2009 cars

Notice: Never attempt to remove the intake manifold from a hot engine, allow the engine to cool to ambient temperature. The intake manifold is made of a composite plastic and can be damaged if it is removed when the engine is hot.

1. Remove the EVAP emission canister valve tube (1).
2. Remove the EVAP emission canister valve (2).
3. Remove the throttle body.
4. Remove fuel pipes and clip. Remove the fuel rail assembly.
5. Remove the intake manifold retaining nuts and bolts.
6. Remove the intake manifold.
7. Remove the intake manifold gasket, if necessary. The gasket can be used again if it is not damaged.
8. If the intake manifold needs to be replaced, transfer the throttle body.

### Removal Procedure

1. Disconnect the fuel pressure regulator hose from the throttle body and fuel rail.
2. Remove the throttle body.
3. Remove the fuel pipes and clip.
4. Remove the fuel rail assembly.
5. Remove the knock sensor connector from the intake manifold.
6. Remove the knock sensor.
7. Remove the intake manifold retaining nuts and bolts.
8. Remove the intake manifold.
9. Remove the intake manifold gasket. The gasket is reusable if it is not damaged.
10. If the intake manifold needs to be replaced, transfer the following parts:

• | The throttle body

• | The body gasket. The manifold to throttle body gasket is reusable if it is not damaged.