For 1990-2009 cars

Action | Normal Results
--- | ---

1. Put the mirror select switch in the LEFT position.
2. Operate the mirror adjustment switch (pad) in up and down.

The left outside mirror should move up and down smoothly.

Operate the mirror adjustment switch (pad) in right and left. | The left outside mirror should move left and right smoothly.

1. Put the mirror select switch in the RIGHT position.
2. Operate the mirror adjustment switch (pad) in up and down.

The right outside mirror should move up and down smoothly.

Operate the mirror adjustment switch (pad) in right and left. | The right outside mirror should move right and left smoothly.