For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Remove the console. Refer to Console Replacement .
3. Using a screwdriver, disconnect the control cable end from the pin on the control assembly.
4. Remove the control cable retaining clip.
5. Depress the tabs on the control cable and remove the cable from the control assembly.
6. Disconnect the control assembly electrical connectors.
7. Remove the control assembly-to-floor pan bolts and remove the control assembly.
8. If the shift control assembly is being replaced, transfer the parts as needed. Refer to the appropriate procedures in this service manual.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the control assembly into the vehicle and install the control assembly-to-floor pan bolts.

Tighten
Tighten the control assembly-to-floor pan bolts to 8 N·m (71 lb in).

2. Connect the control assembly electrical connectors.
3. Connect the control cable to the pin on the control assembly.
4. Secure the control cable into the control assembly by pushing into place.
5. Install the control cable retaining clip.
6. Install the console. Refer to Console Replacement .
7. Enable the SIR system. Refer to Enabling the SIR System .