For 1990-2009 cars

### Removal Procedure

1. Remove the door lock switch. Refer to Door Lock Switch Replacement - Front
2. Remove the power mirror switch on the driver side door. Refer to Power Mirror Switch Replacement
3. Using a small flat-bladed tool, remove the tweeter cover.
4. Remove the upper door trim panel. Refer to Upper Extension Trim Panel Replacement
5. Remove the fastener cover from the inner pull handle.
6. Remove the fasteners.
7. Remove the pull handle.

### Installation Procedure

1. Install the pull handle to the door.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the fasteners to the pull handle.

Tighten
Tighten the fasteners to 2 N·m (17.7 lb in).

3. Install the cover to the fasteners.
4. Install the upper door trim panel. Refer to Upper Extension Trim Panel Replacement .
5. Install the tweeter cover.
6. Install the power mirror switch on the driver side door. Refer to Power Mirror Switch Replacement
7. Install the door lock switch. Refer to Door Lock Switch Replacement - Front