For 1990-2009 cars

### Removal Procedure

1. Operate the sunroof to the ¼ open position.
2. Remove the 4 screws from the "U" cover.
3. Close the sunroof
4. Remove the "U" cover by unsnapping the sides and lower the cover down into the passenger compartment.
5. Remove the 4 bolts from the encapsulated glass.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the encapsulated glass with the 4 bolts.

Tighten
Tighten the encapsulated glass-to-sunroof module fasteners to 4 N·m (35 lb in).

2. Align the encapsulated glass to the roof in the 4 locations indicated by the arrows, 0-1 mm (0-3/64 in) lower than the roof in the front and 0-1 mm (0-3/64 in) higher than the roof in the rear.
3. Install the "U" cover by snapping the sides to the sunroof assembly.
4. Operate the sunroof to the ¼ open position.
5. Install the 4 screws to the "U" cover.

Tighten
Tighten the sunroof module "U" cover retaining screws to 4 N·m (35 lb in).

6. Verify a smooth operation.
7. Verify the alignment to the roof.