For 1990-2009 cars

### Removal Procedure

1. Partially remove the center trim plate by pulling at the clip locations to disengage the clips. Twist the trim plate sideways to access the back of trim plate.
2. Disconnect the center trim plate switch connections and remove the center trim plate.
3. Remove the center trim plate switch by disengaging the attaching clips.

### Installation Procedure

1. Install the center trim plate switches by snapping it into place.
2. Connect the wiring harnesses to the trim plate switches.
3. Position the center trim plate and secure it to the instrument panel by gently pushing at the attaching clip locations.