For 1990-2009 cars

### Removal Procedure

1. Open the front and rear doors.
2. Remove the push-in retainers from the top of the rocker panel molding.
3. Remove the push-in retainers from the bottom of the rocker panel molding.
4. Remove the push-in retainers and the rear wheelhouse liner to rocker panel molding.
5. Remove the push-in retainers and the front wheelhouse liner to rocker panel molding.
6. Remove the rocker panel molding, rotating out and down from the rocker panel.

### Installation Procedure

1. Position the rocker panel molding to the rocker panel.
2. Install the push-in retainers to the top of the rocker panel molding.
3. Install the push-in retainers to the bottom of the rocker panel molding.
4. Install the push-in retainers and the rear wheelhouse liner to rocker panel molding.
5. Install the push-in retainers and the front wheelhouse liner to rocker panel molding.
6. Close the front and rear doors.