For 1990-2009 cars

## Taillamps, Turn Signal, Stoplamps and Back-up Lamps Sedan

1. Open the trunk.
2. Pull back the interior trim.
3. Rotate the bulb socket being replaced counter-clockwise 1/4 of a turn pressing the socket in firmly. Pull the socket rearward until the bulb clears the taillamp housing.
4. Replace it with the appropriate bulb.

## Taillamps, Turn Signal, Stoplamps and Back-up Lamps Wagon

1. Open the liftgate.
2. Remove the interior access trim panel.
3. Rotate the bulb socket being replaced counter-clockwise 1/4 of a turn pressing the socket in firmly. Pull the socket rearward until the bulb clears the taillamp housing.
4. Replace it with the appropriate bulb.