For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Disconnect the camshaft position (CMP) sensor harness connector.
3. Remove the knock sensor 2 pigtail from the attachment clip.
4. Remove the CMP sensor attachment bolt and remove the sensor.

### Installation Procedure

1. Install the knock sensor 2 pigtail clip to the CMP sensor if installing the new sensor.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the CMP sensor by gently pushing into place and install the attachment bolt.

Tighten
Tighten the camshaft position sensor bolt to 8 N·m (71 lb in).

3. Insert the knock sensor 2 pigtail to the clip.
4. Connect the CMP sensor harness connector. Push the connector in until the lock position is felt, then pull back to confirm engagement.