For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the front door water deflector, starting at the top, pull downward.

### Installation Procedure

1. Route the electrical connectors through the existing holes in the water deflector.
2. Install the water deflector to the door inner panel by aligning it to the door. Use a roller around the outer edgeof the deflector to ensure proper seating.
3. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .