For 1990-2009 cars

### Removal Procedure

1. Partially remove the I/P filler, knee bolster, by pulling at the attaching clip locations near the top.
2. Remove the upper and lower I/P cluster trim plate fasteners and pull rearward to remove the cluster trim plate.
3. Disconnect the solar load sensor wire next to the radio area.
4. Remove the top trim cover of the solar load sensor with a small blade tool.
5. Using your finger nail or small blade tool separate the outer/lower shell from the inside sensor while pulling upward and remove the solar load sensor. The outer/lower shell will not be removed.
6. Remove the wire by aligning the connector end carefully with the outer/lower shell to remove.

### Installation Procedure

1. Feed the solar load sensor wire through the instrument panel.
2. Snap the solar load sensor in place.
3. Snap the trim cover on the solar load sensor.
4. Connect the solar load sensor wire.
5. Install the I/P cluster trim plate and the fasteners.

Tighten
Tighten the I/P cluster trim plate-to-I/P housing fasteners to 2.5 N·m (22 lb in).

6. Install the I/P filler, knee bolster, by snapping the bolster in place.