For 1990-2009 cars

## Rear Compartment Floor Panel Carpet Replacement Sedan

### Removal Procedure

1. Remove the rear seat backs.
2. Remove the rear compartment floor carpeting.

### Installation Procedure

1. Position the rear compartment floor carpet into the vehicle.
2. Position the carpet behind the lowered rear seat backs.
3. Raise the rear seat backs.

## Rear Compartment Floor Panel Carpet Replacement A

### Removal Procedure

1. smvis77749aa

Flip the rear compartment floor carpet away from the side carpet.

2. Remove the rear compartment side carpet fasteners.
3. Remove the side carpet assembly.

### Installation Procedure

1. smvis77748aa

Position the side carpet to the vehicle.

2. Install the side carpet fasteners.
3. Position the decklid weatherstrip over the rear compartment side carpet.
4. Position the floor carpet into place.