For 1990-2009 cars

Caution: When using power tools that may create smoke when cutting urethane sealant, work should be done in a well ventilated area and/or with a NIOSH/MSHA Approved air supplied respirator to prevent possible harmful exposure.

When the urethane adhesive is heated enough to give off smoke, high levels of methylene diisocyanate (MDI) may be present. Unprotected exposure to methylene diisocyanate (MDI) may result in severe, chronic, debilitating respiratory problems.

Caution: When replacing stationary windows, use Urethane Adhesive Kit GM P/N 12346392 (Canadian P/N 10952983), or a urethane adhesive system meeting GM Specification GM3651G, to maintain original installation integrity. Failure to use the urethane adhesive kit will result in poor retention of the window which may allow unrestrained occupants to be ejected from the vehicle resulting in personal injury.

### Adhesive Service Kit

Refer to Adhesive Service Kit Description .