For 1990-2009 cars

### Removal Procedure

1. Open and support the hood.
2. Remove the hood secondary latch lever rivet by using a metal saw or a cut-off wheel.
3. Remove the rivet, the spring, and the lever.

### Installation Procedure

1. Install the hood secondary latch lever, the spring, and the rivet.
2. Flatten the end of the rivet to secure in place by using clamp-nose vise grip pliers or a hammer and dolly.
3. Inspect the secondary latch for proper operation.