For 1990-2009 cars

1. Remove the accessory drive belt tensioner bolt.
2. Remove the accessory drive belt tensioner.
3. Remove the engine front cover bolts.
4. Remove the long water pump bolt.
5. Remove the engine front cover and gaskets.
6. Remove the crankshaft front cover oil seal with an appropriate tool.

1. Remove the accessory drive belt tensioner.
2. Remove the engine front cover bolts.
3. Remove the water pump bolt.
4. Remove the engine front cover and gaskets.
5. Remove the crankshaft front cover oil seal using an oil seal removal tool.