For 1990-2009 cars

## Instrument Panel Air Outlet Vent Replacement Left Side

### Removal Procedure

1. Remove the left side lower I/P closeout panel (hush panel) retainers and let closeout panel hang loose.
2. Remove the I/P filler knee bolster by pulling at the attaching clip locations.
3. Remove the left side A/C vent fastener and partially remove vent.
4. Disconnect the electrical connection from the interior lamp dimmer switch.

### Installation Procedure

1. If the left side A/C vent is being replaced, transfer the interior lamp dimmer switch to new vent.
2. Connect the electrical connection to the interior lamp dimmer switch.
3. Install the left side a/C vent fastener.

Tighten
Tighten the A/C outlet to 2.5 N·m(22 lb in).

4. Install the I/P filler knee bolster
5. Install the left side lower I/P closeout (hush panel) with retainers.

## Instrument Panel Air Outlet Vent Replacement Right Side

### Removal Procedure

1. Position the HVAC vent to the upward most position.
2. Pull outward at the bottom of the HVAC vent to unsnap the vent from the housing.

### Installation Procedure

1. Position the vent into the housing with HVAC vent vanes facing downward. Snap it into position.
2. Operate the vent to ensure the proper function.