For 1990-2009 cars

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Remove the rivets from the fascia outer reinforcement.
3. Remove the fascia outer reinforcement from the fascia.

### Installation Procedure

1. Position the fascia outer reinforcement onto the fascia.
2. Install the rivets to the fascia outer reinforcement.
3. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .