For 1990-2009 cars

### Removal Procedure

1. Pull up on the control lever boot to disengage from the console.
2. Cut the plastic tie strap that secures the boot to the shift lever.
3. Remove the control lever boot.

### Installation Procedure

1. Install the boot assembly to the lever so the plastic tie strap is in the groove on the lever.
2. Pull the tie strap tight with pliers.
3. Pull the control lever boot down and snap the boot into the console opening.