For 1990-2009 cars

### Removal Procedure

1. Remove the front seat assembly. Refer to Front Seat.
2. INSERT GRAPHIC SMVIS 80875AA1

Remove the front seat back cover. Refer to Front Seat Back Cover/Pad.

3. Remove the lumbar adjuster cable fasteners from the seat frame.
4. Unhook the lumbar assembly from the retainers and remove the lumbar assembly.

### Installation Procedure

1. Hook the lumbar mechanism into the retainers.
2. Route the lumbar adjuster cable and the adjuster to the seat side frame.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the lumbar adjuster with the fasteners.

Tighten
Tighten the lumbar adjuster fasteners to 3 N·m (27 lb in).

4. Insert graphic SMVIS 80875AA1

Install the front seat cover assembly. Refer to Front Seat Pad/Cover.

5. Install the front seat assembly. Refer to Front Seat.