For 1990-2009 cars

#### Tools Required

SA9303BR Stop Lamp Switch Adjustment Gage

Use the CD changer/player magazine SA9303BR . Insert it to the right of the magazine line-up arrows (1). Insert the metal tool straight in until only approximately 1 inch is still exposed. Then gently angle the tool. This motion will move the locking tab forward (2), which results in the CD Changer/Player releasing the magazine.

If a CD in the magazine is blocking the magazine from ejecting all the way out:

• | If the harness is the reason that the CD Changer/Player does not have power, try to find another harness to connect the CD Changer/Player to power. If none are available, have the CD Changer/Player and remaining CDs serviced as an assembly.

• | If the problem is internal to the CD Changer/Player, have the CD Changer/Player, magazine, and any remaining CDs serviced as an assembly.