For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the steering wheel. Refer to Steering Wheel Replacement .
3. Remove the SIR coil. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement .
4. Remove the upper and lower shrouds. Refer to Steering Column Trim Covers Replacement .
5. Depress the lock tabs on the left and right multi-function levers. Remove the multi-function levers.
6. Disconnect the housing electrical connectors.
7. Remove the housing form the steering column.

### Installation Procedure

1. Slide the bracket onto the column.
2. Hand tighten the lower bolt until snug.
3. Hand tighten the upper bolt until snug.

Notice: Refer to Fastener Notice in the Preface section.

4. Tighten the lower bolt.

Tighten
Tighten the bolt to 8 N·m (71 lb in).

5. Tighten the upper bolt.

Tighten
Tighten the bolt to 8 N·m (71 lb in).

6. Connect the ignition housing electrical connectors.

Important: Ensure that both locking tabs are seated.

7. Install the multi-function levers.
8. Install the upper and lower shrouds. Refer to Steering Column Trim Covers Replacement .

Tighten
Tighten the shroud screws to 4 N·m (35 lb in).

9. Install the SIR coil. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement .
10. Install the steering wheel. Refer to Steering Wheel Replacement .
11. Connect the negative battery cable.