For 1990-2009 cars

### Removal Procedure

Important: Remove each bolt on each cap one turn at a time until there is no spring tension on the camshaft.

1. Remove the exhaust camshaft bearing cap bolts.
2. Remove the camshaft bearing caps ensuring they are marked and refitted in the same position on the assembly.
3. Remove the exhaust camshaft.

Important: Keep all of the roller finger followers and valve lash adjusters in order so that they can be reinstalled in their respective locations.

4. Remove the exhaust camshaft roller finger followers.
5. Remove the hydraulic element adjusters.