For 1990-2009 cars

## Child Restraint Tether Anchor Replacement Sedan

### Removal Procedure

1. Remove the rear shelf panel. Refer to the Rear Window Shelf Trim Panel Replacement in Interior Trim.
2. Remove the child restraint bracket fastener and remove the bracket.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the child restraint bracket with the bolt.

Tighten
Tighten the bolt to 20 N·m (15 lb ft).

2. Install the rear shelf panel. Refer to Rear Window Shelf Trim Panel Replacement in Interior Trim.

## Child Restraint Tether Anchor Replacement Wagon

### Removal Procedure

1. Remove the load floor panel from the vehicle.
2. Remove the child restraint bracket fastener and remove the bracket.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the child restraint fastener and the bracket to the vehicle.

Tighten
Tighten the bracket bolt to 20 N·m (15 lb ft).

2. Install the load floor panel.