For 1990-2009 cars

The following table lists the parameters displayed by the scan tool. The parameters are displayed by ABS/TCS data, switch inputs, exterior lamps, interior lamps, door locks, wiper/washer, and security data groups.

Scan Tool Displays
Parameter | Unit
--- | ---
ABS/TCS Data
Battery 1 | Volts
Traction Active | Yes/No
Traction Control Status | On/Off
ABS Fault | Yes/No
Traction LED Command | On/Off
Traction LED Feedback | High/Low
Park Brake Switch | On/Off
Switch Inputs
Battery 1 | Volts
Driver Door Switch | High/Low
Passenger Door Switches | High/Low
Key In Ignition | Yes/No
Decklid Ajar Switch | High/Low
Oil Life Reset Switch | High/Low
Park Brake Switch | On/Off
Low Coolant | Yes/No
Low Brake Fluid | Yes/No
A/C Request | Yes/No
High Beam Input = Off | Yes/No
High Beam Input = DRL | Yes/No
High Beam Input = High | Yes/No
Low Beam Switch | On/Off
Park Lamp Switch | On/Off
Lock Switch | On/Off
Unlock Switch | On/Off
Front Wiper Switch | On/Off
Rear Wiper Switch | On/Off
Rear Defog Switch | On/Off
Rear Defog Relay Command | On/Off
Rear Defog Relay Feedback | High/Low
Shifter Unlock Command | On/Off
Shifter Unlock Feedback | High/Low
Exterior Lamps
Battery 1 | Volts
High Beam Input | Volts
High Beam Input = Off | Yes/No
High Beam Input = DRL | Yes/No
High Beam Input = High | Yes/No
Low Beam Switch | On/Off
Park Lamp Switch | On/Off
DRL Relay Command | On/Off
DRL Relay Feedback | High/Low
Interior Lamps
Battery 1 | Volts
Inadvertent Lamp Power Command | On/Off
Inadvertent Lamp Power Feedback | High/Low
Dome Lamp Command | On/Off
Dome Lamp Feedback | High/Low
Driver Door Switch | High/Low
Pass Door Switches | High/Low
Key In Ignition | Yes/No
Instrument Panel Dimmer Input | Volts
I/P Dimmer Output | % DC
Door Locks
Battery 1 | Volts
Driver Unlock Relay Command | On/Off
Driver Unlock Relay Feedback | High/Low
Pass Unlock Relay Command | On/Off
Pass Unlock Relay Feedback | High/Low
Lock All Relay Command | On/Off
Lock All Relay Feedback | High/Low
Remote Lock Command | Yes/No
Remote Unlock Command | Yes/No
Remote Panic Command | Yes/No
Remote Trunk Command | Yes/No
Remote Programmed | Yes/No
Lock Switch | On/Off
Unlock Switch | On/Off
Trunk Release Switch | On/Off
Trunk Release Solenoid Feedback | High/Low
Trunk Release Solenoid Command | On/Off
Wiper/Washer
Battery 1 | Volts
Wiper Delay Input | Volts
Wiper Delay 1 | Yes/No
Wiper Delay 2 | Yes/No
Wiper Delay 3 | Yes/No
Front Wiper Switch | On/Off
Front Wiper Relay Command | On/Off
Front Wiper Relay Feedback | High/Low
Rear Wiper Switch | On/Off
Rear Wiper Relay Command | On/Off
Rear Wiper Relay Feedback | High/Low
Front Washer Motor Input | On/Off
Rear Washer Motor Input | On/Off
Washer Fluid Level | Low/OK
Security Data
Battery 1 | Volts
Ignition 1 Input | High/Low
Accessory | High/Low
Passlock Input | Volts
Passlock Power Feedback | High/Low
Key Learned | Yes/No
Key Learned Enabled | Yes/No
Security LED | On/Off/Flash
Horn Relay Command | On/Off
Horn Relay Feedback | High/Low
Passlock Timer | Seconds
Auto-Learn Timer | Seconds
Decklid Ajar Switch | Low/High
Trunk Release Switch | On/Off