For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster trim panel. Refer to Driver Knee Bolster Panel Replacement .
2. Remove the retaining screw.
3. Remove the deflector assembly.
4. Disconnect the electrical connector.
5. Remove the deflector from the instrument panel (I/P).

### Installation Procedure

Important: If you are replacing the old deflector with a new deflector, transfer the switch to the new deflector.

1. Connect the electrical connector.
2. Position the deflector to the I/P.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the retaining screw.

Tighten
Tighten the screw to 2 N·m (18 lb in).

4. Install the knee bolster trim panel. Refer to Driver Knee Bolster Panel Replacement .