For 1990-2009 cars

### Removal Procedure

1. Remove the front fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the plastic fasteners at the outer edge of the fascia lower support to the front bumper impact bar.
3. Remove the fascia lower support from the front bumper impact bar.

### Installation Procedure

1. Position the fascia lower support to the front bumper impact bar.
2. Install the plastic fasteners attaching the fascia lower support to the front bumper impact bar.
3. Install the front fascia. Refer to Front Bumper Fascia Replacement .