For 1990-2009 cars

### Removal Procedure

1. Remove the engine coolant temperature sensor.
2. Remove the thermostat and water feed pipe retaining bolts.

Important: Twist the water feed pipe while pulling to remove it from the water pump.

3. Remove the thermostat housing and water feed pipe from the water pump.

Important: Be sure to remove the bolt that goes through the front of the engine block.

4. Remove the water pump retaining bolts.
5. Remove the water pump assembly.