For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment floor carpet. Refer to Rear Compartment Floor Panel Carpet Replacement .
2. Remove the rear compartment side carpet fasteners.
3. Remove the side carpet assembly.

### Installation Procedure

1. Position the side carpet to the vehicle.
2. Install the side carpet fasteners.
3. Position the decklid weatherstrip over the rear compartment side carpet.
4. Install the rear compartment floor carpet. Refer to Rear Compartment Floor Panel Carpet Replacement .