For 1990-2009 cars

### Removal Procedure

1. Move the front seat to the forward position.
2. Remove the carpet retainer molding in the area surrounding the center pillar lower molding by pulling at the attaching clip locations.
3. Using a trim tool, remove the outside center pillar weatherstrip.

Important: Care must be taken not to drop fasteners in the center pillar structure.

4. Remove the shoulder belt height adjuster fasteners.

Important: Care must be taken not to drop fasteners in the center pillar structure.

5. Remove the shoulder belt retractor fastener access plug.
6. Remove the shoulder belt retractor fastener.

Important: Upper and lower moldings will stay attached to each other while being removed.

Important: Shoulder belt assembly and height adjuster unit will stay attached to the center pillar upper and lower moldings when the moldings are removed.

7. Starting at the top, gently pull on the center pillar upper molding to disengage the attaching clips.
8. Pull on the center pillar lower molding to disengage the attaching clips.
9. Remove the shoulder belt from the shoulder belt retainer.
10. Remove the safety belt guide fastener and remove the guide.

### Installation Procedure

1. Install the safety belt guide with a fastener.

Tighten
Tighten the Safety Belt Guide Fasteners to 1.5 N·m (13 lb in).

2. Position the shoulder belt behind the shoulder belt retainer.
3. Attach the center pillar molding assemblies to the vehicle by firmly pushing at the clip locations.
4. Install the retractor fastener.

Tighten
Tighten the retractor fastener to 35 N·m (26 lb ft).

5. Install the retractor plug.
6. Install the height adjuster fasteners.

Tighten
Tighten the height adjuster fasteners to 35 N·m (26 lb ft).

7. Install the center pillar outside weatherstrip.
8. Install the carpet retainer by gently pushing at the attaching clip locations.
9. Install the weatherstrip over the center pillar lower molding and the rocker panel molding using a flat blade tool.
10. Function the shoulder belt to ensure the proper operation.
11. Place the front seat in the original position.