For 1990-2009 cars

### Gear Teeth Counts and Ratios

| GEAR TEETH COUNT
--- | ---
1st Drive: | 13
1st Driven: | 44
2nd Drive: | 25
2nd Driven: | 44
3rd Drive: | 39
3rd Driven: | 46
4th Drive: | 47
4th Driven: | 42
5th Drive: | 54
5th Driven: | 38
Reverse Drive: | 25
Reverse Idler: | 21
1st & 2nd Gear Synchronizer Sleeve: | 49
Output Shaft | 20
Ring Gear: | 89

### Blocking Ring Clearances

MEASUREMENT | STANDARD | SERVICE LIMIT
--- | --- | ---
| METRIC | ENGLISH | METRIC | ENGLISH
1st and 2nd Gears | 1.2-1.4 mm (min.) | 0.047-0.055 in. (min.) | 0.8 mm (min.) | 0.032 in (min.)
3rd, 4th, and Reverse Gears | 0.9-1.2 mm (min.) | 0.035-0.047 in. (min.) | 0.5 mm (min.) | 0.020 in (min.)
5th Gear | 0.7-1.1 mm (min.) | 0.028-0.043 in. (min.) | 0.5 mm (min.) | 0.020 in. (min.)

### Axial Play Specifications

MEASUREMENT | SPECIFICATION
--- | ---
| METRIC | ENGLISH
Between 2nd and 3rd Drive Gears | 0.05 mm-0.40 mm | 0.002 in.-0.016 in.
Between 4th Drive Gear and Input Shaft Bearing | 0.05 mm-0.40 mm | 0.002 in.-0.016 in.
Between Reverse Gear and Reverse Gear Washer | 0.10 mm-0.20 mm | 0.004 in.-0.008 in.
Input Shaft Axial Play | 0.09 mm-0.15 mm | 0.004 in.-0.006 in.
Output Shaft Axial Play | This is a calculated value, it can change based upon age of case and output shaft bearing, refer to "Transaxle Assembly" in this service manual.