For 1990-2009 cars

### Removal Procedure

1. Remove the CHMSL cover by gently pulling on the CHMSL cover assembly.
2. Remove the liftgate trim panel retainers in the upper corner locations.
3. Pull the liftgate trim panel out at the upper corner locations.
4. Starting from the top, disengage the attaching clips by gently pulling on the liftgate upper molding.

### Installation Procedure

1. Position the liftgate upper molding at the attaching clip locations.
2. Gently push at the attaching clip locations to secure the upper molding to the liftgate.
3. Install the CHMSL cover by gently pushing at the attaching clip locations.
4. Install the liftgate trip panel retainers in the upper corner locations.