For 1990-2009 cars

### Removal Procedure

1. Remove the front screw from the front of the outer belt seal.
2. Release the rear of the outer belt seal from the clip retainer.
3. Remove the outer belt seal from the door by firmly pulling up.

### Installation Procedure

1. Press the outer belt seal down onto the flange until fully seated.

Press the rear of the outer belt seal onto the clip retainer.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the screw to the outer belt seal.

Tighten
Tighten the screw to 2 N·m (18 lb in).