For 1990-2009 cars

# RKE Transmitter is Inoperative or Intermittently Inoperative

Subject: | Remote Keyless Entry (RKE) Transmitter is Inoperative or Intermittently Inoperative -- Diagnose and Repair as Necessary Using the Diagnostic Information Contained in This Bulletin

Models: | 2000 Saturn L-Series vehicles equipped with RKE (RPO AU0) and L81 (V-6) engines built before VIN YY664721 -- 2000 Saturn L-Series vehicles equipped with RKE (RPO AU0) and L61 (4-Cylinder) engines built before VIN YY665426

### Condition:

Some customers may comment that the remote keyless entry (RKE) transmitter is inoperative or intermittently inoperative.

### Cause:

Flux residue from the circuit board soldering process may interrupt the electrical connection between the transmitter circuit board and the negative side of the transmitter battery.

### Correction:

Refer to the Remote Keyless Entry (RKE) System Check diagnostic chart within this bulletin for further diagnostic information.

### Parts Requirements:

Part Number | Description
--- | ---
24401698 | Transmitter Asm -- R/Con Dr Lk
CR2032 or equivalent | Battery -- Panasonic 3 volt
*Available locally or through Digi Key by calling 1-800-344-4539

### Claim Information:

To receive credit for this repair during the warranty coverage period, submit a claim through the Saturn Dealer System for R4490 Transmitter, Remote Door/ Rear Compartment Lock -- Replace. If another procedure is performed, refer to the appropriate Electronic Labor Time Guide for the correct Labor Operation Code and Time.