For 1990-2009 cars

### Front Door Striker

1. Using a grease pencil, mark around the striker for installation purposes.
2. Remove the bolts.
3. Remove the striker and striker shim if present.

### Installation Procedure

1. Loosely install the striker and striker shim, if present, with the bolts.
2. Align the striker with the marks made prior to removal.
3. Hand tighten the bolts.
4. Inspect the door closing. Align the striker as required.

Notice: Refer to Fastener Notice in the Preface section.

5. Tighten the striker bolts.

Tighten
Tighten the door striker bolts to 20 N·m (15 lb ft).