For 1990-2009 cars

1. Remove the engine coolant temperature sensor.
2. Remove the water pipe support bracket and bolts.
3. Remove the thermostat and water feed pipe retaining bolts.

Important: Twist the water feed pipe while pulling to remove it from the water pump cover.

4. Remove the thermostat housing and water feed pipe from the water pump cover.
5. Remove the water pump retaining bolts. Be sure to remove the bolt that goes through the front of the engine block.
6. Remove the water pump assembly.

### Removal Procedure

1. Remove the engine coolant temperature sensor.
2. Remove the thermostat and water feed pipe retaining bolts.

Important: Twist the water feed pipe while pulling to remove it from the water pump.

3. Remove the thermostat housing and water feed pipe from the water pump.

Important: Be sure to remove the bolt that goes through the front of the engine block.

4. Remove the water pump retaining bolts.
5. Remove the water pump assembly.