For 1990-2009 cars

#### Tools Required

• | J 8062 Valve Spring Compressor

• | J 36017 Valve Guide Seal Remover

• | J 43963 Valve Spring Compressor (off car)

1. Remove the coolant air bleed hose fitting.

Important: Ensure that the valve train components are kept together and identified in order for proper re-installation in their original position.

2. Using the J 8062 and the J 43963 , compress the valve spring.
3. Remove the valve keys.
4. Slowly release the J 8062 and the J 43963 from the valve spring assembly.
5. Remove the retainer.
6. Remove the spring.

Notice: Do not damage the valve guide. Remove any burrs that have formed at the key groove by chamfering the valve stem with an oil stone or a file.

7. Remove the valve seal. Use the J 36017 . Do not reuse.
8. Remove the valve.
9. Remove the remaining valves.
10. Remove the cylinder head plugs.

#### Tools Required

• | J 8062 Valve Spring Compressor

• | J 36017 Valve Guide Seal Remover

• | J 43963 Valve Spring Compressor Adapter

1. Remove the coolant air bleed hose fitting.

Important: Ensure that the valve train components are kept together and identified in order for proper re-installation in their original position.

2. Using the J 8062 and the J 43963 , compress the valve spring.
3. Remove the valve keys.
4. Slowly release the J 8062 and the J 43963 from the valve spring assembly.
5. Remove the retainer.
6. Remove the spring.

Notice: Do not damage the valve guide. Remove any burrs that have formed at the key groove by chamfering the valve stem with an oil stone or a file.

7. Remove the valve seal. Use the J 36017 . Do not reuse.
8. Remove the valve.
9. Remove the remaining valves.
10. Remove the cylinder head plugs.