For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise the vehicle on the hoist.
2. Remove the wheel and tire assemblies.
3. Remove the exhaust muffler hangers.
4. Remove the heat shield from the rear suspension.
5. Remove the left and right rear stabilizer bar links to the rear axle control arm bolts.
6. Remove the stabilizer bar tot he rear suspension attachment fasteners.
7. Remove the stabilizer bar from the vehicle.

### Installation Procedure

Important: If installing onto a new crossmember, loosen the bolt and re-tighten to specification.

1. Install the stabilizer bar into the vehicle and tighten the stabilizer bar clamp fasteners.

Tighten
Tighten the rear stabilizer bar clamp-to-cross member to 55 N·m (41 lb ft).

2. Install the stabilizer bar links to the rear axle control arm.

Tighten
Tighten the rear stabilizer bar-to-knuckle to 55 N·m (41 lb ft).

3. Install the exhaust muffler hangers.
4. Install the heat shield to the rear suspension support.

Tighten
Tighten the heat shield-to-rear suspension support to 8 N·m (71 lb in).

Notice: Refer to Wheel Installation Caution in the Preface section.

5. Install the wheel and tire assemblies onto the hub.
6. Install the wheel bolts and tighten in a star pattern.

6.1. | Hand tighten all 5 wheel bolts.

6.2. | Use a torque wrench to tighten the wheel bolts using a star pattern.

Tighten
Tighten the wheel bolts first pass to 63 N·m (46 lb ft).

6.3. | Use a torque wrench to final tighten the wheel bolts using a star pattern.

Tighten
Tighten the wheel bolts final pass to 125 N·m (92 lb ft).

7. Lower the vehicle from the hoist.