For 1990-2009 cars

### Removal Procedure

1. Remove the transaxle. Refer to "Transaxle Removal" procedure in this service manual.
2. Remove the hydraulic line from the slave cylinder.
3. Remove the hydraulic line from the slave cylinder.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the slave cylinder. Use LOCTITE 592® P/N 21485278 thread sealant on the screws.

Tighten
Tighten the slave cylinder fasteners to 10 N·m (89 lb in).

2. Connect the hydraulic line to the slave cylinder.
3. Bleed the slave cylinder. Refer to Clutch Slave Cylinder Bleeding.
4. Install the transaxle. Refer to "Transaxle Installation" in this service manual.