For 1990-2009 cars

### SIR System

This vehicle is equipped with the supplemental inflatable restraint (SIR) system. Refer to Disabling and Enabling the SIR system in SIR.

### Electrostatic Discharge (ESD)

The remote keyless entry (RKE/Security System) is a subsystem of the body control module (BCM). This system has components which are sensitive to electrostatic discharge (ESD). ESD can damage many solid state components. Not all components that are susceptible to damage from ESD are labeled with the ESD precautionary symbol. Exercise caution when handling all solid state electrical components.

Avoid damaging solid state components by taking the following precautions:

• | Discharge personal electricity by touching a metal ground point after sliding across the vehicle seat, sitting, rising or walking.

• | Do not touch the exposed electrical terminals on a component with your fingertip or tool. The connector that you are checking may be tied into a circuit that is susceptible to damage by ESD.

• | Do not allow a screwdriver or similar tool to contact the exposed terminals when disconnecting a connector.

• | Do not remove the protective packaging of the solid state component until you are ready to install the solid state component.

• | Unless specified in a particular diagnostic procedure, avoid jumping components or connectors, grounding components or connectors or using the test equipment probes on the components or connectors.

• | When a diagnosis requires the use of test equipment probes, connect the ground lead first.

• | Touch the solid state component's package to a ground before opening the package.

• | Do not lay the solid state component on a metal workbench or on top of an electrically operating appliance or piece of equipment.

• | Do not drop the solid state component.

### Visual/Physical Inspection

One of the most important checks, prior to performing any diagnostic activity, is a careful visual inspection of the complaint related wiring and components. This can often lead to fixing a malfunction without any further steps. Inspect the battery charge level (green eye) to ensure the battery is not discharged. Inspect for blown fuses. Inspect all the related vacuum and electrical circuits for pinches, cuts or disconnects. A good visual inspection is very important.

### General Service

The diagnostic flow charts contained in this manual are used to find and repair the malfunctions which the self-diagnostics of the module have found. If a diagnostic trouble code (DTC) is a history DTC, the malfunction may be intermittent. Try wiggling the wiring and connectors as this can often cause the malfunction to appear. It is not recommended to replace the modules based on history codes.

It is recommended to use a scan tool in performing the system diagnostics. The scan tool displays will assist in diagnosing RKE/security system related malfunctions. The diagnostic flow charts in this section rely on data from a scan tool to make repair decisions.