For 1990-2009 cars

1. Remove the remaining twelve bolts (9, 12 and 16) from the control valve body assembly (18).
2. Remove the control valve body assembly (18).
3. Remove and discard the valve body to spacer plate gasket (22).

1. Remove the remaining twelve bolts (9, 12 and 16) from the control valve body assembly (18).
2. Remove the control valve body assembly (18).
3. Remove and discard the valve body to spacer plate gasket (22).