For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
A/C Compressor Clutch Coil Fasteners | 5 N·m | 44 lb in
A/C Compressor Clutch Plate Bolt | 12 N·m | 9 lb ft
A/C Outlet-to-I/P Fasteners | 2.5 N·m | 22 lb in
Audio System Amplifier-to-I/P Beam Fasteners | 10 N·m | 89 lb in
Battery Terminal Bolts | 17 N·m | 13 lb ft
Blower Motor Control Module | 3.0 N·m | 27 lb in
Blower Motor Housing Screws | 1.0 N·m | 9 lb in
Blower Motor Resistor Card Fastener Automatic Climate Control Vehicles Only: | 1.0 N·m | 9 lb in
Blower Motor Resistor Screws | 1 N·m | 9 lb in
Cluster Trim Plate-to-I/P Cluster Fasteners | 2.2 N·m | 22 lb in
Compressor-to-Engine Block Bolts | 22 N·m | 17 lb ft
Condensate Drain Tube Bolt | 3.5 N·m | 31 lb in
Condenser Block-to-Radiator End Tank Bolt | 5 N·m | 44 lb in
Condenser-to-Radiator Bolts | 5 N·m | 44 lb in
Console Fasteners | 2.5 N·m | 22 lb in
Control Head to I/P Screws | 2.5 N·m | 22 lb in
Discharge Line Clamp Fastener-to-Cradle | 5 N·m | 44 lb in
Discharge Line-to-Compressor Bolt | 16 N·m | 12 lb ft
Discharge Line-to-Condenser Block Bolt | 20 N·m | 15 lb ft
Evaporator Core Service Door-to-HVAC Module Fasteners | 1 N·m | 9 lb in
Fan Housing-to-Blower Motor Housing Screws | 1 N·m | 9 lb in
Filter Housing Screws | 3.5 N·m | 31 lb in
Filter Housing-to-HVAC Module Fasteners | 3.5 N·m | 31 lb in
Front of Dash Screen-to-Front of Dash Fasteners | 1 N·m | 9 lb in
Glove Compartment Bin-to-I/P Fasteners | 2.5 N·m | 22 lb in
Glove Compartment Door Fasteners | 2 N·m | 18 lb in
HVAC Center Duct-to-HVAC Module Fastener | 1 N·m | 9 lb in
HVAC Module Duct Screws | 1.0 N·m | 9 lb in
HVAC Module Screws | 1.0 N·m | 9 lb in
HVAC Module-to-Front of Dash Bolts | 4.5 N·m | 40 lb in
Heater Core Retaining Strap Screw | 1.0 N·m | 9 lb in
Heater Primary Lever Fastener | 1.0 N·m | 9 lb in
I/P Attachment Fasteners | 20 N·m | 26 lb ft
I/P Beam Inner Studs | 20 N·m | 15 lb ft
I/P Beam Outer Bolts | 7 N·m | 62 lb in
I/P Beam-to-Steering Column Brace Nuts | 20 N·m | 15 lb ft
I/P Bracket Nuts | 20 N·m | 15 lb ft
I/P Bracket-to-Floor Panel Nuts | 20 N·m | 15 lb ft
I/P Cluster Trim Plate-to-I/P Housing Fasteners | 2.5 N·m | 22 lb in
I/P Screws to Radio | 2.5 N·m | 22 lb in
Instrument Cluster-to-I/P Housing Fasteners | 2.3 N·m | 22 lb in
Liquid Line Clamp Fasteners-to-Condenser | 6 N·m | 53 lb in
Liquid Line-to-Condenser Block Bolt | 20 N·m | 15 lb ft
Lower Fan Shroud Retaining Nuts | 5 N·m | 44 lb in
Mode Actuator Fastener | 1.0 N·m | 9 lb in
Nut to Harness Clip | 6 N·m | 53 lb in
Pressure Relief Valve-to-Compressor | 12 N·m | 9 lb ft
Pressure Transducer-to-Suction/Liquid Line | 7 N·m | 62 lb in
Radio-to-I/P Fasteners | 2.5 N·m | 22 lb in
Rear Shoulder Belt-to-C-Pillar | 35 N·m | 26 lb ft
Receiver/Dehydrator Block Bolts | 3 N·m | 27 lb in
Receiver/Dehydrator Clamp Bolt | 5 N·m | 44 lb in
Recirculation Actuator Bracket-to-HVAC Module Screws | 1.0 N·m | 9 lb in
Seat Attachment Fasteners | 25 N·m | 19 lb ft
Shoulder Belt-to-Seat Frame Bolts | 35 N·m | 26 lb ft
Splash Shield-to-Wheelhouse and Cradle Fasteners | 5 N·m | 44 lb in
Steering Column Attachment Fasteners | 30 N·m | 20 lb ft
Steering Column Intermediate Shaft Pinch Bolt | 30 N·m | 20 lb ft
Steering Column Trim Cover Fasteners | 4 N·m | 35 lb in
Steering Wheel Attachment Nut | 40 N·m | 30 lb ft
Suction Liquid Line Assembly Clamps | 5 N·m | 44 lb in
Suction Liquid Line-to-Liquid Line | 12 N·m | 9 lb in
Suction Pipe-to-Compressor Bolt | 16 N·m | 12 lb ft
Suction/Liquid Line Assembly Clamp-to-Horn Bracket Nut | 10 N·m | 89 lb in
Suction/Liquid Line Assembly Clamps | 5 N·m | 44 lb in
Suction/Liquid Line Assembly-to-TXV Bolt | 7 N·m | 62 lb in
Suction/Liquid Line-to-Liquid Line | 12 N·m | 9 lb ft
Suction/Liquid Line-to-Suction Pipe Nut | 12 N·m | 9 lb ft
TXV-to-Block Bolts | 7 N·m | 62 lb in
Valve Assembly-to-Service Port Base Fastener | 12 N·m | 106 lb ft
Vent Primary Lever Fastener | 1.0 N·m | 9 lb in
Wiper Arm Assembly Nuts | 12 N·m | 9 lb ft
Wiper Module Bolts | 5 N·m | 44 lb in