For 1990-2009 cars

1. Remove the transmission filter assembly (85).
2. Remove the oil level control valve (86).

Notice: Do not damage the case sealing surface when removing the filter seal assembly.

3. Using a chisel, indent top of seal to relax press fit of seal.
4. Using a small screwdriver remove the filter neck seal (84) from the transmission case. The filter neck seal (84) is not reusable and should be discarded.