For 1990-2009 cars

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Turn the fascia over and release the pressure clips at the outside edge of the filler.
3. Remove the filler from the fascia.

### Installation Procedure

1. Install the filler to the rear bumper fascia.
2. Ensure that the pressure clips are in the proper location.
3. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .