For 1990-2009 cars

The heated oxygen sensor (HO2S) bank 1 sensor 2 is threaded into the cylinder 1, 3, 5 exhaust pipe behind the pre-converter (cylinders 1, 3 and 5 are closest to the front of the dash). The sensor is an electrical source that responds to oxygen content out of the pre-converter. When the sensor reaches approximately 316°C (600°F), it produces a voltage based on the difference in oxygen between the atmosphere and exhaust gas. The ECM sends a bias voltage (421-479 mV) on the signal line, which is pulled up through high resistance. When the HO2S bank 1 sensor 2 is cold, it produces no voltage and has extremely high internal resistance. The internal resistance of the sensor is much greater than the resistance of the bias pull-up resistor. However, when the sensor heats up, it produces voltage that overrides the bias voltage. This voltage is read by the ECM to determine the efficiency of the catalytic converter. Under normal conditions, low sensor voltage means high oxygen content/lean air-fuel mixture and vice versa. Normal sensor readings at steady cruise with a properly functioning catalytic converter will be around 500-800 mV. DTC P0136 sets when the HO2S bank 1 sensor 2 signal voltage is too low for a certain length of time.

### DTC Parameters

DTC P0136 will set if HO2S bank 1 sensor 2 voltage is less than 40 mV when:

• | The condition exists for longer than 1 minute and 20 seconds.

• | The Engine is running.

• | The HO2S bank 1 sensor 2 is in a closed loop.

• | The Fuel level is greater than 10%.

• | The calculated converter temperature is less than 940°C (1724°F).

• | The commanded air/fuel ratio is 14.7 to 1.

• | The Battery voltage is greater than 11.0 volts.

• | There is no EVAP purge solenoid or the EVAP system DTCs have been set.

DTC P0136 diagnostic runs continuously once the above conditions have been met.

P0136 is a type B DTC

To locate an intermittent problem, use the scan tool to monitor the HO2S BANK 1 SENSOR 2 voltage with the engine idling at normal operating temperature. Wiggling the wires while watching for a change in HO2S BANK 1 SENSOR 2 voltage may locate the area where a short to ground in the wiring could lie.

Important: Do not apply grease or any material in the HO2S bank 1 sensor 2 harness connector or alter the wiring in any way. The wires carry air reference to the sensor used to determine the difference in oxygen between the exhaust gas and atmosphere.