For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat shoulder belt cover to expose the shoulder belt fastener.
2. Remove the shoulder belt fastener and the shoulder belt.
3. Lower the rear seat back.
4. Route the shoulder belt out of the C-pillar trim at access slot.
5. Remove the C-pillar trim assembly by pulling gently at the C-pillar trim clip locations.

### Installation Procedure

1. Position the C-pillar trim to the vehicle.
2. Install the C-pillar trim by pushing gently at the clip locations.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the rear seat shoulder belt to the C-pillar.

Tighten
The rear shoulder belt upper fasteners to 35 N·m (26 lb ft).

4. Install the rear seat shoulder belt fastener cover.
5. Route the shoulder belt into the C-pillar trim at the access slot.
6. Raise the rear seat back.
7. Function the rear seat shoulder belt to ensure proper operation.