For 1990-2009 cars

1. Install the engine front cover with a new gasket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the long water pump bolt.

Tighten
Tighten the water pump bolt to 25 N·m (18 lb ft).

3. Install the engine front cover bolts.

Tighten
Tighten the engine front cover bolts to 25 N·m (18 lb ft).

4. Install the accessory drive belt tensioner.
5. Install the accessory drive belt tensioner bolt.

Tighten
Tighten the bolt to 45 N·m (33 lb ft).

### Installation Procedure

1. Install the engine front cover and new gasket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the long water pump bolt.

Tighten
Tighten the water pump bolt to 25 N·m (18 lb ft).

3. Install the engine front cover bolts.

Tighten
Tighten the front cover-to-block bolts to 25 N·m (18 lb ft).

4. Install the accessory drive belt tensioner.

Tighten
Tighten the drive belt tensioner bolt to 45 N·m (33 lb ft).