For 1990-2009 cars

### Removal Procedure

1. Remove the pull handle fastener cap.
2. Using a small flat-bladed tool, remove the tweeter cover.
3. Remove the door lock switch to expose the pull handle fastener.
4. Remove the upper door trim panel. Refer to Upper Extension Trim Panel Replacement .
5. Remove the fastener from the pull handle.
6. Remove the door lock switch from the pull handle. Refer to Door Lock Switch Replacement .
7. Remove the pull handle from the door.

### Installation Procedure

1. Install the pull handle to the door.
2. Install the door lock switch to the pull handle. Refer to Door Lock Switch Replacement .

Notice: Refer to Fastener Notice in the Preface section.

3. Install the fasteners to the pull handle.

Tighten
Tighten the fasteners to 2 N·m (17.7 lb in).

4. Install the upper door trim panel. Refer to Upper Extension Trim Panel Replacement .
5. Install the door lock switch to the pull handle.
6. Install the tweeter cover.
7. Install the cap to the pull handle fastener.