For 1990-2009 cars

### Removal Procedure

1. Remove the lower right side dash closeout panel, hush panel.
2. Remove the lower right side air duct.
3. Remove the lower right side console closeout panel.
4. Remove the radio trim bezel and the electrical connections.
5. Remove the radio and tilt the radio downward and lay the radio in front of the console.
6. Remove the aspirator hose.

### Installation Procedure

Important: Failure to connect the aspirator hose securely may result in automatic climate control performance problems.

1. Connect the aspirator hose.
2. Install the radio.
3. Install the radio trim bezel and the electrical connections.
4. Install the lower right side console closeout panel.
5. Install the lower driver's side console closeout panel.
6. Install the lower driver's side air duct.
7. Install the lower driver's side dash closeout panel, hush panel.